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DISCLAIMER AND SCOPE LIMITATIONS
	IMPORTANT NOTICE — PLEASE READ BEFORE USING THIS REPORT
This report has been prepared using GeoScreen®, an automated ground risk screening platform developed and operated by Magnum GSI Ltd.

The report provides an indicative, desk-based assessment of ground conditions and associated constraints based solely on the interrogation and interpretation of publicly available datasets, including but not limited to British Geological Survey (BGS), Scottish Environment Protection Agency (SEPA), Mining Remediation Authority (MRA), Historic Environment Scotland (HES), and NatureScot data sources.

This report:
•  DOES NOT constitute a professional geotechnical assessment or a BS 5930:2015+A1:2020 compliant desk study
•  DOES NOT include intrusive ground investigation, site walkover, or statutory searches
•  IS informed by general principles derived from relevant UK geotechnical guidance, but does not constitute a desk study compliant with BS 5930:2015+A1:2020
•  IS intended solely for early-stage feasibility, due diligence, and preliminary risk screening purposes

The findings presented are indicative only. Site-specific ground conditions may vary and can only be reliably established through an appropriately scoped ground investigation and professional interpretation by a suitably qualified and experienced geotechnical engineer.




1   SITE INFORMATION AND CONTEXT
The site is located at KY1 1XT, within the administrative area of Fife Council. The OS National Grid Reference (NGR) is 327747 E, 691406 N. This Ground Risk Snapshot has been prepared in the context of Residential development.

2   DATA SOURCES ASSESSED
The following publicly available datasets were interrogated automatically during preparation of this Ground Risk Snapshot. All data were collected on 18 October 2026.

	Data Source
	Information Provided

	Ordnance Survey (OS) Names API
	Geocoding, site location, Local Planning Authority (Appendix A)

	BGS 1:625,000 Bedrock Geology WMS
	Bedrock geology and formation identification (Appendix B)

	BGS 1:625,000 Superficial Deposits WMS
	Superficial geology and drift deposits (Appendix C)

	BGS Faults OGC API
	Fault lines within 1 km of site

	BGS SOBI Borehole Database
	Proximate borehole records (SOBI)

	BGS Radon Potential WMS
	Radon potential class and protective measures flag (Appendix H)

	SEPA flood maps (river and coastal, ArcGIS REST)
	Flood likelihood extents (Appendix D)

	SEPA flood maps - surface water and small watercourses
	Surface water flood depth and extent (Appendix L)

	Scottish Water Water Supply Catchments and SEPA Drinking Water Protected Area catchments
	Public water supply catchment check - surface-water supplies (Appendix M)

	SEPA granted authorisations (ArcGIS REST) and SEPA landfill register + council historic landfill records. Contains public sector information licensed under the Open Government Licence v3.0. Source: waste sites and capacity data tool (Scottish Environment Protection Agency). Copyright City of Edinburgh Council, contains Ordnance Survey data © Crown copyright and database right (2026). Contains OS data © Crown copyright and database right 2026 and Scottish local authority data from the Spatial Hub.
	Landfill sites within 500 m. Data reflects SEPA and council records at the time this report was generated and may be subject to change (e.g. new or updated permits). SEPA's records cover landfill sites licensed since 1996, including sites whose licence has ended. Council historic landfill records are published by only a minority of Scottish councils; where a council publishes none, landfill sites that closed before 1996 may be present that are not recorded.

	Mining Remediation Authority (MRA) open data (OGL v3). Contains Mining Remediation Authority information © Mining Remediation Authority, 2026
	Coal Mining Reporting Area, mining risk class (Appendix G)

	Historic Environment Scotland designations (local dataset)
	Listed buildings (Category A/B/C), scheduled monuments, conservation areas, Inventory gardens and designed landscapes, and Inventory battlefields within 500 m (Appendix E)

	NatureScot and Scottish Government (ArcGIS REST)
	SSSIs, SACs, SPAs, Ramsar sites, NNRs, National Scenic Areas, and National Parks within 2 km (Appendix F)

	BGS 1km Non-Coal Mining Hazard Hex Grid v8
	Non-coal underground mining hazard classification (Appendix G)

	OpenStreetMap (local extract, amenity=fuel)
	Petrol filling stations within 500 m (Appendix O)

	Scottish Public Sector LiDAR - DTM tiles (0.25-1m, AWS Open Data)
	Site topography, terrain descriptor, slope analysis (Appendix N)

	SEPA Granted Authorisations (permits: waste, PPC, radioactive substances and water discharges; ArcGIS REST) + OpenStreetMap fuel forecourts
	Environmental permits, registered facilities and flood defence assets within 1 km (Appendix O). Data reflects SEPA and council records at the time this report was generated and may be subject to change (e.g. new or updated permits).

	GB1900 Historical Gazetteer (CC-BY-SA 4.0, Great Britain Historical GIS / GB1900 partners and volunteers)
	Historical map feature and tunnel/subway portal positioning, OS Six-Inch County Series 1888-1913 (Appendix P, Q)

	OpenStreetMap (local extract, infrastructure and land-use sites)
	Current infrastructure and land-use feature positioning (Appendix P)

	OpenStreetMap (local extract, tunnel/subway geometry)
	Underground and buried structure positioning (Appendix Q)

	SEPA Future Flood Maps – River, Coastal and Surface Water (climate change)
	Flood extent with climate change, reference only (Appendix R) – does not affect the ratings in the table above



3   GEOHAZARD RISK SUMMARY
The table below summarises the geohazard risk rating and data confidence level for each hazard assessed. The overall ground risk classification for the site is High.

	Ref.
	Geohazard
	Risk Rating
	Data Confidence

	GH01
	Mining Legacy (Appendix G)
	High
	High

	GH02
	Compressible Ground
	Medium
	Medium

	GH03
	Shrink-Swell Clays
	Low
	Medium

	GH04
	Slope Instability
	Low
	Low

	GH05
	Dissolution Features
	Medium
	Medium

	GH06
	Made Ground
	Medium
	Medium

	GH07
	River and Coastal Flood Risk (Appendix D)
	High
	High

	GH08
	Surface Water Flood Risk (Appendix L)
	High
	High

	GH09
	Radon (Appendix H)
	Low
	High

	GH10
	Ground Gas
	Medium
	Medium

	GH12
	Aggressive Ground Conditions
	Medium
	Medium

	PWS
	Public Water Supply Catchment (Appendix M)
	Not identified
	High



The overall risk classification reflects the highest-rated hazard, with adjustment where multiple Medium-rated hazards collectively indicate increased development sensitivity at this preliminary screening stage.
Flood-risk ratings reflect the worst case anywhere within the route supplied for this Tier 0 screening. Mapped flood extents may also be present in the surrounding area outside the route. Flood zones and surface water extents have been checked across the whole of the route; the Tier 1 report gives the share of the site affected.

4   RISK RATING AND CONFIDENCE DEFINITIONS
4.1   Risk Rating Scale
	Risk Rating
	Description

	Very High
	A major geohazard has been identified at or close to the site. Development is feasible subject to appropriate mitigation of the identified geotechnical risks and subject to confirmation by intrusive ground investigation.

	High
	A significant geohazard has been identified that is likely to influence the development. Targeted ground investigation and specialist assessment are recommended.

	Medium
	A geohazard has been identified that may influence the development. Mitigation measures may be required; targeted investigation is advisable to confirm or refine the rating.

	Low
	No significant geohazard has been identified from available data at this desk-based stage. No specific mitigation measures are anticipated at this stage, subject to confirmation by ground investigation.


4.2   Data Confidence Level
	Confidence Level
	Definition

	High
	Multiple corroborating data sources; data returned successfully with high spatial resolution and dataset coverage at this location.

	Medium
	Single primary data source; partial data available; some spatial uncertainty or limited dataset coverage. Rating reflects most probable scenario.

	Low
	Limited data available; API query returned no data or fell back to default. Treat the rating with caution and verify through further investigation.



5   SEPA AUTHORISED PERMITTED FACILITIES AND FUEL STATIONS
SEPA-authorised permitted facilities and OpenStreetMap fuel stations identified within 1km of the route are listed below. See Appendix O for mapped locations.
	Facility Name
	Category / Type
	Distance
	Direction

	Wider study area - 100 m to 1 km from the site (4 facilities)

	Esso
	Active fuel forecourt
	128m
	N (Ch 0+672)

	Wemyssfield Service Station
	Industrial activity (PPC Part B)
	299m
	S (Ch 0+246)

	Kirkcaldy STW, Pathhead Headworks, Kirkcaldy
	Sewage treatment works
	769m
	N (Ch 1+515)

	Hutchison's Mill, East Bridge, Kirkcaldy, KY1 2SR
	Industrial installation (PPC Part A)
	802m
	N (Ch 1+515)




	GROUND RISK KEY TAKEAWAY

	The site is assessed as High geotechnical risk, driven by Mining Legacy, River and Coastal Flood Risk, and Surface Water Flood Risk, each rated High, with Compressible Ground, Dissolution Features, Made Ground, Ground Gas, and Aggressive Ground Conditions as additional Medium-rated considerations. A GeoScreen Tier 1 Preliminary Ground Risk Screening Report is recommended for detailed geohazard narrative, site investigation recommendations, and a Conceptual Site Model.





6	LIMITATIONS AND LIABILITY STATEMENT
	This report has been prepared using GeoScreen®, an automated ground risk screening platform developed and operated by Magnum GSI Ltd, for the sole benefit of the named client, Magnum GSI, for the specific purpose of preliminary, indicative desk-based appraisal of land at KY1 1XT (route c. 1.51 km, 10 m corridor).

The report is based entirely on a desk-based review, drawing upon publicly available information, mapping, and datasets as listed in Section 4. No intrusive investigations, physical site inspection, utilities searches, ecological surveys, or statutory authority searches have been undertaken. Accordingly, actual site conditions may differ materially from those described.

The findings and opinions expressed in this report are indicative and do not constitute a guarantee of planning permission, development feasibility, ground conditions, environmental status, or contamination status. The risks identified are perceived risks based on available information and are not exhaustive. Actual risks can only be assessed through site-specific intrusive investigation and professional interpretation.

This report has been generated using automated, rule-based analysis. AI-assisted interpretation is used solely to generate the short Ground Risk Key Takeaway summary above; all geohazard ratings and other report content are produced by deterministic, rule-based logic, not AI narrative. It does not constitute site-specific advice issued by a Chartered Geotechnical Engineer or other qualified professional, and should be read alongside the limitations set out in this section.

This report has been prepared exclusively for the named client. No responsibility or liability is accepted for reliance placed on this report by any third party — including purchasers, lenders, solicitors, planners, designers, or contractors — without prior written consent.

The information contained herein reflects the state of publicly available data at the time of automated data retrieval on 18 October 2026. No obligation is accepted to update this report for subsequent changes in circumstances, legislation, published datasets, or guidance.

To the fullest extent permitted by law, GeoScreen® and Magnum GSI Ltd accept no liability for any loss, damage, cost, or expense arising from the use of this report beyond its stated purpose or intended use.

This report should not be relied upon as a substitute for a professional geotechnical desk study prepared and signed off by a Chartered Geotechnical Engineer in accordance with BS 5930:2015+A1:2020, nor for site-specific ground investigation or planning advice.


6.1	Limitations of Automated Assessment
This report has been generated using an automated, algorithm-based system which applies rule-based logic to available digital datasets. AI-assisted interpretation is limited to generating the short Ground Risk Key Takeaway summary from the automated findings.
While reasonable care has been taken in the development and operation of this platform:
•  The assessment is inherently probabilistic in nature
•  Not all site-specific hazards, anomalies, or constraints may be identified
•  The system may not capture localised conditions or site-specific variations that are not represented in underlying datasets
Accordingly, the report should be treated as a screening tool only, and not as a substitute for professional advice.
6.2	Data Sources and Accuracy
All information used in the preparation of this report is obtained from third-party data providers.
Magnum GSI Ltd:
•  Does not independently verify the accuracy, completeness, or currency of underlying datasets
•  Accepts no responsibility for errors, omissions, or inaccuracies within source data
•  Makes no representation that all relevant datasets or constraints have been identified
The report reflects the state of data at the time of retrieval only, and no obligation is accepted to update the report for subsequent changes.
6.3	Reliance and Use
This report is produced solely for the benefit of the named client for the stated purpose.
It:
•  Should not be relied upon solely for design, planning submission, construction, or investment decisions without appropriate professional advice and intrusive ground investigation
•  Should not be used as a substitute for a professional desk study or geotechnical investigation
•  Should only be used as part of a wider risk assessment process
•  Must not be altered, redacted, or modified from the version as originally delivered; the version delivered by email and archived by Magnum GSI Ltd constitutes the definitive record
Any decisions taken based on this report are made at the sole risk of the user. This report must not be reproduced, distributed, or relied upon by any party other than the named commissioning client without the prior written consent of Magnum GSI Ltd. This does not prevent the client sharing this report, unmodified, with professional advisers directly engaged on the Site (for example, an architect, planning consultant, lender, or contractor instructed by the client) for purposes connected with that engagement; such sharing does not extend any duty of care to, or permit reliance by, the recipient (see Section 6.5).
6.4	Professional Advice
Outputs generated by GeoScreen®:
•  Do not constitute site-specific advice issued by a Chartered Geotechnical Engineer
•  Do not replace the requirement for professional input in accordance with BS 5930:2015+A1:2020, Eurocode 7, and NPF4 requirements
Professional services, including detailed desk studies, ground investigations, and geotechnical design advice, should be commissioned where required.
Where this report is commissioned by or reviewed by a qualified geotechnical engineer or engineering geologist, that professional is responsible for applying independent judgement when interpreting these findings and for meeting their own duty of care when advising clients.
6.5	Liability
Nothing in this Section 6.5 excludes or limits liability for death or personal injury caused by negligence, fraud or fraudulent misrepresentation or any other liability that cannot lawfully be excluded or limited.
To the fullest extent permitted by law:
•  Magnum GSI Ltd shall not be liable for any indirect, consequential, or economic loss arising from reliance upon this report, and accepts no liability for any loss, damage, cost, or expense arising from the use of this report beyond its stated purpose or intended use
•  No duty of care is owed to any third party, and no reliance may be placed upon this report by any party other than the named client without prior written consent of Magnum GSI Ltd
•  The report is provided on an “as is” basis without warranty, express or implied. No warranty is given that all risks, constraints, or site conditions have been identified
Where liability cannot be lawfully excluded, the total liability of Magnum GSI Ltd shall not exceed the cap set out in Clause 12.1 of the Company’s Terms of Service (available at geoscreen.uk) in effect at the date of this report.



APPENDICES
Map extracts are provided for indicative purposes only. All maps are generated from publicly available data sources as listed in Section 4. Users should refer to the original data sources for authoritative information. Scales and extents are approximate.
Appendix A:	Site Location Plan
OS base mapping showing site location and surroundings
[image: ]

Appendix B:	BGS Bedrock Geology Extract
BGS 1:625,000 bedrock geology at site location
[image: ]

Appendix C:	BGS Superficial Geology Extract
BGS 1:625,000 superficial deposits at site location
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Appendix D:	SEPA Flood Map Extract (River and Coastal)
SEPA flood map likelihood classification
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Appendix E:	Heritage Designations (Historic Environment Scotland)
Listed buildings, scheduled monuments and conservation areas within 500m
[image: ]

Appendix F:	Ecological Designations (NatureScot)
SSSI, SAC, SPA, Ramsar, National Scenic Area and National Park designations within search radii
[image: ]

Appendix G:	Mining Remediation Authority Output
MRA development risk and mine entries data
[image: ]

Appendix H:	BGS/UKHSA Radon Potential Extract
Radon potential classification at site location
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Appendix I:	Historical OS Mapping (1885–1903)
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Appendix J:	Historical OS Mapping (1888–1913)
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Appendix K:	Historical OS Mapping (1919–1947)
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Appendix L:	Surface Water Flood Risk (SEPA)
[image: ]
Appendix M:	Public Water Supply Catchments (Scottish Water / SEPA)
[image: ]
Appendix N:	Site Topography — Scottish Public Sector LiDAR Digital Terrain Model
[image: ]
Appendix O:	Permitted Regulated Facilities — SEPA Granted Authorisations
[image: ]
Appendix P:	Historical & Current Map Features
[image: ]
Appendix Q:	Underground & Buried Structures
[image: ]
Appendix R:	Flood Risk – Reference (Climate Change)
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